# WL-330gE

## 4-in-one portable wireless router

Innovative Integration of Access Point, Ethernet Adapter, Gateway and Universal Repeater

Model Number : N50 >

### Specifications

Network Standard | IEEE802.11g, IEEE802.11b, IEEE802.11d, IEEE802.3, IEEE802.3u, IEEE802.1X, WPA, WMM, IPv4
Interface | 1 * RJ45 for 10/100 Base-T with auto cross-over function (MDI/MDI-X)
Antenna | Internal*2 IFA antenna
Operating Frequency | 2.4GHz
Operation Channel | 11 for N. America, 14 Japan, 13 Europe (ETSI) 3 (non-overlapping)
Data Rate | 802.11g: 6, 9, 12, 18, 24, 36, 48, 54Mbps 802.11b: 1, 2, 5.5, 11Mbps
Output Power | 19dBm(FCC regulation) or 17dBm(CE regulation) in b/g mode with 1.5dB tolerance
LED Indicator | Ethernet, Wireless (WiFi Association), PWR Wireless Association: On: client associated (AP/Gateway/Bridge/Repeater mode), or associated to AP with strong signal (Client mode, RSSI >= -65 dBm) Flashing: (Client mode) < -89 dbm On:200ms, Off:1000ms · >= -89 dbm < -83 dbm On:200ms, Off:800ms >= -83 dbm < -77 dbm On:200ms, Off:600ms >= -77 dbm < -71 dbm On:200ms, Off:400ms >= -71 dbm < -65 dbm On:200ms, Off:200ms Off: client not associated (AP/Gateway/Bridge/Repeater mode), or not associate to AP (Client mode)
Modulation | OFDM, CCK, DQPSK, DBPSK
Range | Indoor 130ft (40m), semi-open 330ft (100m) Outdoor (LOS, Light of Sight) 1500ft (457m) The range may vary by different environment
Management | Operation mode: AP, Client, URE, Gateway Guest SSID DHCP server, DHCP client DNS Proxy, Automatic IP, PPPoE, PPTP login client support, Static IP, Big Pond login client support Static Route, NTP support, UPnP, DDNS (DynDNS, ZoneEdit, TZO Save/restore configuration files Upgrades via web browser & Bootloader Firmware restoration WMM SSID Isolation: Support SSID hiding Firmware Restoration
Utilities | Device Discovery: Discover all ASUS AP/Gateway in network and help user to invoke Web Configuration page. Firmware Restoration: Restore firmware while system enters rescue mode.
Receiver Sensitivity | B MODE (-95dBm@1Mbps,-96dBm@2Mbps,-95dBm@5.5Mbps,-92dBm@11Mbps) G MODE(-94dBm@6Mbps,-93dBm@9Mbps,-91dBm@12Mbps,-90dBm@18Mbps,-86dBm@24Mbps,-83dBm@36Mbps,-77dBm@48Mbps,-74dBm@54Mbps)
Security | Firewall: NAT and SPI (Stateful Packet Inspection) Virtual DMZ Filtering: Single Port and Port Range, URL based Logging: Syslog Encryption: 64/128-bit WEP WPA-PSK TKIP/AES, WPA2-PSK TKIP/AES, WPA TKIP/AES, WPA2 TKIP/AES, WPA Enterprise, WPA2 Enterprise Authentication: MAC address Access Control, Radius with 802.1 (TLS, TTLS, PEAP)
Physical Specifications | Dimensions：86 mm (L)* 62 mm (W)* 17 mm (H) Weight：50g (Device Only)
Power Adapter | AC Input: 100V~240V (50~60HZ); DC Output: 5V with max. 1 A current
Certifications | CE, FCC, ICE, MIC, C-Tick, NCC
Environmental Specification | Operating Temperature: 0°C to 40°C (32°F to 104ºF) Storage Temperature: -10° to 70° C (-14°F to 158°F) Operating Humidity: 10% to 90% RH (Non-condensing) Storage Humidity: 0% to 90% RH (Non-condensing)
Package Contents | ASUS Portable Wireless AP (WL-330gE)*1 Universal power adapter and plug (5V/1A, 100V~240V)*1 USB power cord*1 RJ45 Cable*1 Travel's bag*1 Support CD (Manual, Utility, GPL)*1 Quick Start Guide*1 Hotspot Mode Instruction*1

Isn´t it so frustrating to find out that the last Internet connection or LAN point has been taken when you just have to access the Internet? Well, fret no more, as ASUS has released the new WL-330gE Wireless Access Point. This nifty little gadget is able to combine 4 wireless functions, namely Access Point, Ethernet Adapter, Gateway and Universal Repeater, into 1 - providing you with connectivity wherever you are. Compact Pocket-size for Portability The ASUS WL-330gE is compact and portable - weighing in at only 2.2 oz and being only 85 mm(L)* 60 mm(W)* 17 mm(H) in size. This petite size makes it easy to carry and implement under any situation and truly makes the ASUS WL-330gE shine. With such portability, it is able to provide wireless access to the Internet easily and without hassle. Numerous Functions To utilize the WL-330gE under AP or Gateway mode, users just have to simply connect it to the Ethernet port on the modem or a LAN connection, and it is ready to go. This is crucial when a meeting room has only one Ethernet connection and there is a need for multiple connections to the Internet. What´s more, the WL-330gE can provide superior flexibility when building a wireless network by supporting NAT and DHCP servers to enable Internet sharing. This is especially useful when you are in an outside hotspot. With the WL-330gE´s "hotspot mode" under the Gateway mode, not only can your laptop access the Internet, your (or your friend´s) other WiFi devices like PDAs, PSPs or WiFi phones can access it as well with no extra cost.
Easy to carry and easy to implement under any circumstance.
In the meeting room: Only one Ethernet cable in the meeting room? Use WL-330gE to share the internet access wirelessly.
In the hotel room: With WL-330gE´s 130ft(40m) indoor range, you can work with your notebook wherever you feel most confortable.
In the hotspot: With WL-330gE´s "hotspot mode" under gateway mode, not only your laptop can get on the internet but your (or your friend´s) other WiFi devices (PDA, PSP, or WiFi phone) can access the Internet without extra cost.
In the office: Under WL-330gE´s Ethernet adapter mode, you can convert all the Ethernet-capable devices (printer, desktop,..) into wireless.
Additionally, in Ethernet adapter mode, the WL-330gE can convert Ethernet-capable devices (desktop, network printer, game console, set top box) into wireless ones. It can even become a universal repeater to extend the wireless signal coverage. Easy and User-Friendly Setup With an easy-to-use setup user interface, you will just require a few clicks to finish setting up for easy wireless Internet access. You only need to find the WL-330gE using "Device Discovery", then click on "Configure" and choose the mode you require, and the WL-330gE is ready to go. Featuring a driver-free Plug´ n´ Play function, Just plug your configured WL-330gE to your modem/router or the Ethernet-capable device, then your WL-330gE is ready to go! Wireless Internet access has never been easier.

### Accessories

- All specifications are subject to change without notice. Please check with your supplier for exact offers. Products may not be available in all markets.
- PCB color and bundled software versions are subject to change without notice.
- Brand and product names mentioned are trademarks of their respective companies.